Basic_data_manipulation_functions
                        Basic data manipulation functions
CAN01AD002              Streamflow data
CAN05AA008              CAN05AA008
CSHShydRology-package   Functions for Canadian hydrological analyses
HYDAT_list              List of Water Survey of Canada hydrometic
                        stations.
Spatial_hydrology_functions
                        Spatial Hydrology functions
StatisticalHydrology-functions
                        Statistical analysis functions
Visualization-functions
                        Visualization functions
ch_axis_doy             Generates the x axis beginning on specified day
                        of year
ch_binned_MannWhitney   Compares two time periods of data using
                        Mann-Whitney test
ch_booth_plot           Create Booth plot of peaks over a threshold
ch_catchment_hyps       Catchment hypsometry
ch_checkcatchment       Check Catchments
ch_checkchannels        Check Channels
ch_circ_mean_reg        Calculates the circular mean, median, and
                        regularity
ch_circular_colors      Color Palettes for Circular
ch_clear_wd             Clear Working Directory
ch_col_gradient         Creates a colour gradient
ch_col_transparent      Add Transparency to plot colours
ch_color_gradient       ch_color_gradient
ch_contours             Create Contours
ch_create_wd            Create working directory
ch_cut_block            Extracts a specified time period from a longer
                        record
ch_date_subset          Subsets dates by string
ch_decades_plot         Plots output from ch_binned_MannWhitney for
                        decades
ch_doys                 Days of year and water year
ch_fdcurve              Plot Flow Duration Curve
ch_ffa_screen_plot      FFA screening plot
ch_flow_raster          Raster plot of daily streamflows
ch_flow_raster_qa       Raster plot of daily streamflows with WSC
                        quality flags
ch_get_ECDE_metadata    Reads Environment Canada Date Explorer (ECDE)
                        meta data file
ch_get_peaks            Extracts peak flows over a threshold
ch_get_url_data         Gets remote data sets
ch_get_wscstation       Reads station information from a data file
                        produced by ECDE
ch_gg_hydrographs       Hydrographs for WSC stations using 'ggplot2'
ch_high_Grubbs_test     Grubbs test for high events
ch_model_hydrograph     Hydrograph plot for model outputs and gauged
                        flows
ch_polar_plot           Polar plot of daily streamflows
ch_polar_plot_peaks     Polar / circular plots of peak flows
ch_polar_plot_prep      Creates a data structure to be passed to
                        'ch_polar_plot'
ch_qa_hydrograph        Plots a hydrograph with the data quality
                        symbols and returns a report on qa symbols and
                        missing data.
ch_read_AHCCD_daily     Reads AHCCD daily file
ch_read_AHCCD_monthly   Reads AHCCD monthly file
ch_read_ECDE_flows      Reads a file of WSC daily flows from
                        ECDataExplorer (ECDE)
ch_regime_plot          Plots the regime of daily streamflows using
                        quantiles
ch_rfa_distseason       Distance in seasonal space
ch_rfa_extractamax      Extracts the annual maxima of a daily time
                        series
ch_rfa_julianplot       Circular plotting by day of year
ch_rfa_seasonstat       Seasonal statistics for flood peaks
ch_sh_get_amax          Extracts annual maximum values from ECDE
                        dataframe.
ch_slice                Converts doy or dwy into a factor that is used
                        to bin data
ch_sub_set_Years        Helper function for selecting points for an
                        axis
ch_tidyhydat_ECDE       Converts a tidyhydat daily flow data tibble to
                        ECDE format
ch_tidyhydat_ECDE_meta
                        Creates an ECDE-like dataframe of metadata from
                        'tidyhydat'
ch_tr_sign              ch_tr_sign
ch_tr_signif            ch_tr_signif()
ch_volcano_pourpoints   Creates a sample file of pour points
ch_volcano_raster       Create Test Raster
ch_wbt_catchment        Delineate catchment boundaries
ch_wbt_catchment_onestep
                        Delineates a catchment in a single step
ch_wbt_channels         Generate stream network
ch_wbt_filenames        Creates names for Whitebox function input and
                        output files
ch_wbt_flow_accumulation
                        Creates flow accumulation grid file
ch_wbt_flow_direction   Creates flow direction grid file
ch_wbt_pourpoints       Snap pour points to channels
ch_wbt_removesinks      Removes sinks from a DEM
ch_wtr_yr               Designation of the water year
flowAtlantic            Annual maxima from sites in the Atlantic region
                        of Canada
